<?xml version="1.0" encoding="ISO-8859-1"?>

<PropertyList>

  <title>Dornier Do X</title>
  <line>________________________</line>
  <key>
    <name>}</name>
    <desc>AutoStart/AutoStop</desc>
  </key>
  <key>
    <name>shift+b (B)</name>
    <desc>Cast Anchor (down)</desc>
  </key>
  <key>
    <name>b</name>
    <desc>Hoist Anchor (up)</desc>
  </key>
  <key>
    <name>s</name>
    <desc>Start engine by engine</desc>
  </key>
  <key>
    <name>Ctrl+s</name>
    <desc>Stop engine by engine</desc>
  </key>
  <key>
    <name>PgUp</name>
    <desc>Increase speed of locked engines</desc>
  </key>
  <key>
    <name>PgDown</name>
    <desc>Decrease speed of locked engines</desc>
  </key>
  <key>
    <name>,</name>
    <desc>Increase speed left locked engines</desc>
  </key>
  <key>
    <name>;</name>
    <desc>Decrease speed left locked engines</desc>
  </key>
  <key>
    <name>.</name>
    <desc>Increase speed right locked engines</desc>
  </key>
  <key>
    <name>:</name>
    <desc>Decrease speed right locked engines</desc>
  </key>
  <key>
    <name>m</name>
    <desc>Increase Mixtures</desc>
  </key>
  <key>
    <name>shift+m (M)</name>
    <desc>Decrease Mixtures</desc>
  </key>
  <key>
    <name>l</name>
    <desc>Interior Lights on/off</desc>
  </key>
  <key>
    <name>c</name>
    <desc>Interior/Exterior View</desc>
  </key>
  <key>
    <name>=</name>
    <desc>Open DO X Engineer Menu</desc>
  </key>
  <key>
    <name> > </name>
    <desc>Switch Pilot/Radio View</desc>
  </key>
  <key>
    <name>shift q (Q)</name>
    <desc>Reset view</desc>
  </key>

  <text>
    _________ Engine control between Pilot and Engineer __________

    In the Middle Panel between the pilot and copilot seat
    you see 12 lamps. 6 left for the larboard engines.
    6 right for the starboard engines.
    The two instruments show you the average rpm of all locked
    engines.

    Red      - engine off
    Yellow   - engine is running but not locked to the two little
    throttle gears of the pilot. Only the engineer
    have the control for this engine in that moment.
    The clutch lever to lock and unlock those engines
    you will find in the Engineer Cabin.
    Green    - pilot have full control over this engine.

    ________________ Navigation with RDF and NDB __________________

    Switch view between Pilot and Radio Navigation Officer with Ctrl-R.
    In the Radio Cabin you will find a RDF-panel. First you have to set
    a NDB, ILS or VOR/DME -frequency in range. Switch on the Instrument with the
    little knob AN/AUS. Fit on the headset and turn the DREHWINKEL-SCHEIBE
    to find the loudest volume of the beacon-signal you have set.
    If you have found the max. volume, click the pencil
    below the RDF-panel.
  </text>

</PropertyList>
