<?xml version="1.0" encoding="ISO-8859-1"?>

<PropertyList>
  
  <title>Dornier Do X</title>
  <key>
    <name> > </name>
    <desc>Switch Copilot/Radio View</desc>
  </key>
  <text>
    ________________ Navigation with RDF and NDB __________________
    
    Switch view between Copilot-Seat and Radio Navigation Seat with Ctrl-R.
    In the Radio Cabin you will find a RDF-panel. First you have to set
    a NDB, ILS or VOR/DME -frequency in range. Switch on the Instrument with the 
    little knob AN/AUS. Fit on the headset and turn the DREHWINKEL-SCHEIBE
    to find the loudest volume of the beacon-signal you have set.
    If you have found the max. volume, click the pencil
    below the RDF-panel. So the pilot get the 
    heading correctino message on his panel.
  </text>
  
</PropertyList>
